**ActiveFloor Boot Procedure**

1. Turn off the power strip connected to the Brightlogic video controller.
2. Shut down the computer
3. Start the computer and Log in as “ActiveFloor” user
4. Wait for everything to boot up and stabilize (About 1 minute)
5. Start the Brightlogic video controller
6. Run the floor startup batch script